**Section 160.160 Piping – Joints**

Joints may be welded or of the ordinary screw type; if of the screw type they shall be screwed together with litharge and glycerine, lamp black or shellac or pipe joint compound.

(Source: Amended at 9 Ill. Reg. 10012, effective October 1, 1985)