**Section 160.180 Piping – Normal Valves**

a) Each pipe attached to a tank shall be provided with a valve at the tank, with no branches nor outlets between the tank and valve.

b) In case two or more tanks are cross-connected, there shall be a valve at each tank in each cross-connection. Tanks with different classes of liquids shall not be cross-connected.