**Section 160.350 Tank Car Unloading Operations – Dome Covers**

After unloading pipe is inserted into dome of tank car and before any pumping is done, the dome shall be tightly covered with wet burlap to limit the release of flammable vapors.

(Source: Amended at 9 Ill. Reg. 10012, effective October 1, 1985)