**Section 160.420 Tank Trucks and Tank Wagons – Double Bulkheads**

Compartment tanks shall be constructed with double bulkheads unless they always carry the same class of liquids in the respective compartments (CLASS I, II, OR III).