**Section 160.425 Tank Trucks and Tank Wagons – No Manifolding of Different Classes of Liquids**

Compartments of tank trucks and tank wagons carrying different classes of liquids shall not be manifolded together. Separate piping and meter where installed shall be provided for each class of liquid to eliminate hazard of mixing.

(Source: Amended at 9 Ill. Reg. 10012, effective October 1, 1985)