**Section 14.820 Design and Layout Requirements**

Every heliport is required to have two defined approach/takeoff paths a minimum of 90° apart. Minimum heliport design and layout requirements shall be in accordance with the standards and limitations shown in Section 14.Appendix G, Illustrations A, B and C, and described in Section 14.Appendix H, Table A.