**Section 16.120 Heliport/Vertiport Surfaces**

a) The Division’s minimum standards for the operation of heliports/vertiports for rotorcraft aircraft are contained in 92 Ill. Adm. Code 14, Aviation Safety.

b) A heliport/vertiport is required to have two defined approach/takeoff paths. The approach path is defined in the heliport/vertiport certificate. The obstruction clearance standards for heliports/vertiports are shown in Section 16.Illustration E.