**Section 178.343 Specification MC 312; Cargo Tanks (Repealed)**

(Source: Repealed at 10 Ill. Reg. 20770, effective December 1, 1986)

**Section 178.343.0.1 [178.343-1] General Requirements (Repealed)**

(Source: Repealed at 10 Ill. Reg. 20770, effective December 1, 1986)

**Section 178.343.0.2 [178.343-2] Thickness of Shell, Heads, Bulkheads, and Baffles of Non-Asme Code Tanks (Repealed)**

(Source: Repealed at 10 Ill. Reg. 20770, effective December 1, 1986)

**Section 178.343.0.3 [178.343-3] Closures for Manholes (Repealed)**

(Source: Repealed at 10 Ill. Reg. 20770, effective December 1, 1986)

**Section 178.343.0.4 [178.343-4] Vents (Repealed)**

(Source: Repealed at 10 Ill. Reg. 20770, effective December 1, 1986)

**Section 178.343.0.5 [178.343-5] Outlets (Repealed)**

(Source: Repealed at 10 Ill. Reg. 20770, effective December 1, 1986)

**Section 178.343.0.6 [178.343-6] Gauging Devices (Repealed)**

(Source: Repealed at 10 Ill. Reg. 20770, effective December 1, 1986)

**Section 178.343.0.7 [178.343-7] Method of Test (Repealed)**

(Source: Repealed at 10 Ill. Reg. 20770, effective December 1, 1986)