PART 428

UNSAFE OPERATING CONDITIONS OF PASSENGER CAR TIRES