**Section 442.216 Child Check System (Optional)**

If a mechanical or electronic child check system is installed, the system must illuminate the interior lights on the bus when the ignition is turned off. (See P.A. 95-0260, effective August 17, 2007.)

(Source: Added at 32 Ill. Reg. 18305, effective November 14, 2008)