**Section 442.265 Seat Belts, Driver's and Passengers'**

a) See the FMVSS for requirements (49 CFR 571.209 and 210).

b) The driver's seat belt assembly shall be arranged so that all portions of the assembly remain above the floor when not in use.

c) If a retractor or retractors are installed, they shall be the emergency locking type.

d) The driver's seat must be equipped with a lap belt/shoulder harness design.

(Source: Amended at 31 Ill. Reg. 8238, effective May 25, 2007)