**Section 442.450 Heater Connections**

Each heater installation shall include two shut off valves as close to the engine inlet and outlet connections as practicable.