**Section 448.50 Official Testing Station Qualifications**

a) The Station shall be clean, orderly, and properly maintained.

b) The Station shall be a permanent building constructed so that the test lane is protected from exposure to the weather. The building shall have a permanent roof, contiguous permanent walls, and a permanent door or doors of sufficient height and width for vehicle passage (see Section 448.70). The floor of the building shall be a level concrete surface.

c) The building shall be located on the Station property so that a vehicle waiting to enter the building shall neither obstruct passing vehicles, nor cause unsafe congestion in an alley, street, or highway.

d) The vehicular entrance and exit to the Station shall neither be obstructed, nor shall a driveway be constructed as to interfere with the free movement of a vehicle entering or exiting the Station Building. The approach to the entrance of the building shall be concrete or asphalt. The incline and/or decline of the approach and exit drives shall not be such as to adversely affect the ingress or egress of any vehicle presented for a safety test.

e) Failure to meet any of the requirements of Section 448.50 shall nullify the application until all the requirements are met.