**Section 451.90 Official Testing Station Requirements**

a) The Station must be clean and properly maintained so that the Station does not interfere with the operation of the test lane or designated testing area.

b) The Station must be a permanent building constructed so that the test lane or designated testing area is protected from exposure to the weather. The building must have a permanent roof, contiguous permanent walls and a permanent door or doors meeting the height and width requirements of this Part (see Section 451.110). The floor of the building must be a level concrete surface.

c) The building must be located on the Station property so that a vehicle waiting to enter the building shall neither obstruct passing vehicles nor cause unsafe congestion in any alley, street or highway.

d) The vehicular entrance and exit to the Station must neither be obstructed nor can a driveway be constructed to interfere with the free movement of a vehicle either entering or exiting the Station building.

e) The approach to the entrance of the Station lane must be concrete, asphalt or a comparable hard surfaced material with minimum dimensions of six feet in length and as wide as the entrance door.

f) Failure to meet any of the requirements of this Section will nullify the application until all requirements are met.

(Source: Amended at 17 Ill. Reg. 12839, effective July 27, 1993)