**Section 451.APPENDIX F Authorized Inspection Equipment**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| CLASS "A," "C," APPLICABLE "B1," "B2," "D" and "P" OTS | | | | |
| Brake Tester | | | Ammco, Tools, Inc. | 900 Flush Type |
| Brake Tester | | | Bear Mfg. Co. | 4505 Surface Type |
| Brake Tester | | | Bear Mfg. Co. | 4506 Flush Type |
| Brake Tester | | | Bear Mfg. Co. | 4510 Surface Type |
| Brake Tester | | | Weaver Mfg. Co. | WY-40SA Surface Type |
| Brake Tester | | | Weaver Mfg. Co. | WY-70SA Flush Type |
| Brake Tester | | | Weaver Mfg. Co. | WY-75 Flush Type |
| Brake Tester | | | Weaver Mfg. Co. | WY-85 Flush Type |
| Brake Tester | | | Weaver Mfg. Co. | WY-400 Surface Type |
| Brake Tester | | | Hunter Engineering Co. | B-400T Computerized |
| Combination Brake Tester – | | | Weaver Mfg. Co. | WY-76 Flush Type |
| Wheel Alignment Tester | | | Weaver Mfg. Co. | WY-86 Flush Type |
|  | | |  |  |
| Wheel Alignment Tester | | | Alemite Division | 3132 Surface Type |
| Wheel Alignment Tester | | | Ammco Tools, Inc. | 8725 Surface Type |
| Wheel Alignment Tester | | | Bear Mfg. Co. | 230 Surface Type |
| Wheel Alignment Tester | | | Bear Mfg. Co. | 231 Flush Type |
| Wheel Alignment Tester | | | Weaver Mfg. Co. | WJ-23 Surface Type |
| Wheel Alignment Tester | | | Weaver Mfg. Co. | WJ-27 Flush Type |
| Wheel Alignment Tester | | | Weaver Mfg. Co. | WJ-132A Surface Type |
| Wheel Alignment Tester | | | Weaver Mfg. Co. | WJ-133A Flush Type |
| Wheel Alignment Tester | | | Weaver Mfg. Co. | WJ-130A Surface Type |
| Wheel Alignment Tester | | | Weaver Mfg. Co. | WJ-131 Flush Type |
| Wheel Alignment Tester | | | Weaver Mfg. Co. | WJ-132 Surface Type |
| Wheel Alignment Tester | | | Weaver Mfg. Co. | WJ-133 Flush Type |
| Wheel Alignment Tester | | | Hunter Engineering Co. | SS 100T |
|  | | | | |
| Lifting Equipment | | | Any Jack, Lift or Hoist having a lifting capacity of 18,000 pounds or more and capable of lifting the heaviest type of vehicle to height adequate for proper "front end" inspection. | |
|  | | | | |
| CLASS "B" AND APPLICABLE "D" and "P" OTS | | | | |
| Brake Tester | | | Ammco Tools, Inc. | 800 Flush Type |
| Brake Tester | | | Bear Mfg. Co. | 450 Surface Type |
| Brake Tester | | | Bear Mfg. Co. | 451 Flush Type |
| Brake Tester | | | Bear Mfg. Co. | 450W Surface Type |
| Brake Tester | | | Weaver Mfg. Co. | WY-30 Surface Type |
| Brake Tester | | | Weaver Mfg. Co. | WY-60 Flush Type |
| \*Combination Brake Tester – Wheel Alignment Tester | | |  |  |
| Weaver Mfg. Co. | WY-25 Surface Type |
| Wheel Alignment Tester | | | Ammco Tools, Inc. | 8725 Surface Type |
| Wheel Alignment Tester | | | Bear Mfg. Co. | 240 Surface Type |
| Wheel Alignment Tester | | | Bear Mfg. Co. | 241 Flush Type |
| Wheel Alignment Tester | | | Bear Mfg. Co. | 250 Surface Type |
| Wheel Alignment Tester | | | John Bean Div. (FMC Corp.) | 146 Surface Type |
| Wheel Alignment Tester | | | John Bean Div. (FMC Corp.) | 149 Surface Type |
| Wheel Alignment Tester | | | Weaver Mfg. Co. | WJ-22 Surface Type |
| Wheel Alignment Tester | | | Weaver Mfg. Co. | WJ-25 Flush Type |
|  | | | | |
| \* | This piece of equipment is acceptable only if it remains in the possession of the owner as of July 1, 1973, or if it is sold to a new owner but remains in the same facility. | | | |
| Lifting Equipment | | Any Jack, Lift or Hoist having a lifting capacity of 5,000 pounds or more and capable of lifting the heaviest vehicle to be inspected to a height adequate for proper "front end" inspection. | | |
|  | | | | |
| The foregoing list of approved equipment supersedes all previous approved equipment lists. | | | | |

(Source: Amended at 17 Ill. Reg. 12839, effective July 27, 1993)