**Section 540.70 Length of Pedestrian Barrier**

As part of the overpass construction, a sufficient length of pedestrian barrier should be erected along the highway to dicourage at-grade crossing and encourage pedestrians to use the overpass. The length of pedestrian barrier and its location will be determined on an individual project basis.