**Section 557.140 Crossing a Roadway (Type II Hazard)**

In determining whether a pupil crossing a roadway is endangered by a serious safety hazard, the type of traffic control, number of lanes, and speed and volume of traffic on the roadway will be considered. To determine whether a hazard exists in a particular situation, appropriate points from subsections (a) and (b) will be added together.

a) Type of Traffic Control

|  |  |  |
| --- | --- | --- |
| CONTROL OF TRAFFIC ON ROADWAY BEING CROSSED | TWO LANES | THREE LANES OR MORE |
| Does Not Stop | 6 points | 8 points |
| Stopped by signals or stop sign | 2 points | 4 points |

b) Speed and Volume of Traffic

|  |  |  |
| --- | --- | --- |
| SPEED | VOLUME | POINTS |
| 50 - 55 mph | Heavy  Moderate  Light | 8  6  4 |
| 40 - 45 mph | Heavy  Moderate  Light | 6  4  2 |
| 30 - 35 mph | Heavy  Moderate  Light | 5  3  1 |

(Source: Amended at 25 Ill. Reg. 16534, effective December 18, 2001)