**Section 1500.210 High Passenger Platforms**

Platforms approximately level with passenger car floors may be constructed and maintained with faces less than 8 feet from the centerline of a subsidiary track used solely for passenger service, provided the coaches served by such platforms are equipped with platform gates which are kept closed while the train is in motion.

(Source: Amended at 29 Ill. Reg. 20360, effective December 15, 2005)