**Section 1500.260 Semaphore Signals**

The distance from the nearest part above the top of rail of a semaphore signal post, other than a dwarf signal, to the centerline of an adjacent main track, shall be not less than 8½ feet. For subsidiary tracks, this distance shall be not less than 8 feet.

(Source: Amended at 29 Ill. Reg. 20360, effective December 15, 2005)