**Section 1535.344 Lenses and Roundels**

Lamp units shall have lenses or roundels, red in color, at least 12 inches in diameter for both front and rear indication. Light transmission values shall conform to current AREMA signal specifications.

(Source: Amended at 29 Ill. Reg. 20376, effective December 15, 2005)