**Section 160.50 Location of Tanks – High Water**

Tanks shall be located and anchored so as to avoid possible damage and flotation from high water in accordance with NFPA #30 2-5.6 (1981).

(Source: Amended at 9 Ill. Reg. 10012, effective October 1, 1985)