**Section 160.370 Truck Loading Operations – Grounding**

Before loading operations begin, tank trucks shall be electrically bonded to pipe line by means of a bonding device at loading dock.