**Section 251.40 Tagging**

a) A certification tag shall be affixed to the side of the portable fire extinguisher or fire suppression system when the extinguisher or system is installed or modified, or when maintenance is performed.

b) All tags that are exposed to the outdoor elements shall be enclosed in a plastic tag protector, unless the tag is made of a weather resistant material.

c) On pre-engineered or engineered fire suppression systems, the certification tag shall be attached and visible at the suppression unit.