**Section 14.730 Obstructions**

In order for an RLA to be eligible for a Certificate of Approval under this Part, an RLA must initially and continually be free of obstructions (e.g., trees, power lines) on all runways or landing strips within the glide ratio and height limitations shown in Appendix E, Illustrations A and C.

(Source: Amended at 38 Ill. Reg. 20064, effective October 2, 2014)