**Section 14.APPENDIX H Heliport/Vertiport Standards, Facility Requirements and Restrictions on Use**

**Section 14.TABLE C Restrictions on Use**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Use | Heliport/ Helistop  Vertiport / Vertistop  Public-Use | Heliport/ Helistop  Vertiport / Vertistop  Private-Use | Heliport/ Helistop  Vertiport / Vertistop  Restricted Landing Area | Hospital Heliport/ Helistop  Vertiport / Vertistop |
| Based Aircraft | No Restrictions | No Restrictions | Maximum of Six Based Helicopters. | Maximum of Six Based Helicopters. |
| Carrying of Passengers for Hire | Allowed | Allowed | Prohibited as Based Operation | EMS only |
| Commercial Maintenance | Allowed for heliports only | Allowed for heliports only | Prohibited | Prohibited |
| Flight Instruction | Unrestricted | Unrestricted | a) Restricted to immediate family of Certificate Holder (excluding cert. held by corp.). Non-continuous.  b) Specialized dual instruction originating from a bonafide flight training operation based at a heliport. | Prohibited |
| Through-the-Fence Operations | Allowed | Not Applicable | Not Applicable | Not Applicable |
| Agricultural Operations | Allowed | Allowed | Allowed | Not Applicable |
| Application of De-icing Agents | Only non-corrosive de-icing agents allowed. | Only non-corrosive de-icing agents allowed. | Only non-corrosive de-icing agents allowed. | Only non-corrosive de-icing agents allowed. |