**Section 442.475 Shock Absorbers**

Two front and two rear heavy-duty double-acting shock absorbers or equivalent damping devices shall be provided.