**Section 460.500 Diesel Emission Inspection 30-Day Warning Notice**

a) *If an annual diesel emission inspection reveals that a vehicle is not in compliance with this Part, the Owner of the Station or the CDET shall issue a warning notice requiring correction of the violation*. [625 ILCS 5/13-109.1] The warning notice shall be in the form of a Diesel Emission Inspection 30-Day Warning Notice, as defined in Section 460.110.

b) *Corrections shall be made and the vehicle submitted to an emission* reinspection at the same Station *that previously issued the warning notice within 30 days from the issuance of the warning notice requiring correction of the violation*. [625 ILCS 5/13-109.1]

c) Examples of basic corrections that will improve diesel emission smoke include, but are not limited to, the following:

1) Replace air filter element, if needed;

2) Check and adjust emission control equipment;

3) Check oil level and ensure correct type recommended for your engine;

4) Tune up, adjust timing, set valve clearance, rack travel, etc.;

5) Ensure correct operation of cooling system;

6) Repair restricted/dented exhaust system; and/or

7) Ensure good grade of fuel.