**Section 1500.130 Subsidiary Passenger Tracks**

a) Except as to ladder tracks the distance between the centerline of any two subsidiary passenger tracks shall be not less than 13 feet.

b) Any pair of subsidiary tracks used solely for passenger service may have centers less than 13 feet provided the centerline of any track, adjacent to either side of such pair of tracks is located not less than 13 feet from the side of the track.

(Source: Amended at 29 Ill. Reg. 20360, effective December 15, 2005)