**Section 1535.345 Signs on Flashing Light Signals**

Where two or more tracks are crossed, the current standard reflector type sign prescribed by AREMA, or as approved by this Commission, indicating the number of tracks shall be placed upon each signal (Appendix B, Illustration E).

(Source: Amended at 29 Ill. Reg. 20376, effective December 15, 2005)