**Section 1535.701 Construction of Barricades**

When by order of the Commission a grade crossing is closed and abolished pursuant to the provisions of Section 18c-7401 of the Law, suitable barricades of neat design shall be constructed in a manner as to prevent use of the crossing by vehicular traffic. The barricades shall be provided with retroreflective material so as to be readily visible during both daylight hours and during nighttime hours in the beam of motor vehicle headlamps. The rail carrier shall be required to pay for the installation of the barricades, and the road authority shall be responsible for all future maintenance.

(Source: Amended at 29 Ill. Reg. 20376, effective December 15, 2005)